|  |  |
| --- | --- |
| 3GPP TS 36.101 V18.10.0 (2025-06) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  Evolved Universal Terrestrial Radio Access (E-UTRA);  User Equipment (UE) radio transmission and reception  (Release 18) | |
|  | |
|  | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2025, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 32

1 Scope 34

2 References 34

3 Definitions, symbols and abbreviations 35

3.1 Definitions 35

3.2 Symbols 37

3.3 Abbreviations 39

4 General 41

4.1 Relationship between minimum requirements and test requirements 41

4.2 Applicability of minimum requirements 41

4.3 Void 41

4.3A Applicability of feature-specific minimum requirements 41

4.4 RF requirements in later releases 43

5 Operating bands and channel arrangement 43

5.1 General 43

5.2 Void 43

5.3 Void 43

5.4 Void 43

5.5 Operating bands 43

5.5A Operating bands for CA 46

5.5B Operating bands for UL-MIMO 67

5.5C Operating bands for Dual Connectivity 67

5.5D Operating bands for ProSe 70

5.5E Operating bands for UE category 0, UE category M1 and M2 and UE category 1bis 71

5.5F Operating bands for category NB1 and NB2 71

5.5G Operating bands for V2X Communication 72

5.5H Operating bands for LTE based 5G terrestrial broadcast 73

5.5K Operating bands for Aerial UE 73

5.6 Channel bandwidth 74

5.6.1 Channel bandwidths per operating band 74

5.6A Channel bandwidth for CA 77

5.6A.1 Channel bandwidths per operating band for CA 79

5.6B Channel bandwidth for UL-MIMO 206

5.6B.1 Void 206

5.6C Channel bandwidth for Dual Connectivity 206

5.6C.1 Void 206

5.6D Channel bandwidth for ProSe 206

5.6D.1 Channel bandwidths per operating band for ProSe 206

5.6F Channel bandwidth for category NB1 and NB2 207

5.6G Channel bandwidth for V2X Communication 208

5.6G.1 Channel bandwidths per operating band for V2X Communication 208

5.6H PMCH bandwidth for LTE based 5G terrestrial broadcast 210

5.6H.1 PMCH bandwidths per operating band for LTE based 5G terrestrial broadcast 211

5.7 Channel arrangement 211

5.7.1 Channel spacing 211

5.7.1A Channel spacing for CA 211

5.7.1F Channel spacing for category NB1 and NB2 211

5.7.1H Channel spacing for LTE based 5G terrestrial broadcast 211

5.7.2 Channel raster 212

5.7.2A Channel raster for CA 212

5.7.2F Channel raster for category NB1 and NB2 212

5.7.3 Carrier frequency and EARFCN 212

5.7.3F Carrier frequency and EARFCN for category NB1 and NB2 215

5.7.3H Carrier frequency and EARFCN for LTE based 5G terrestrial broadcast 216

5.7.4 TX–RX frequency separation 216

5.7.4A TX–RX frequency separation for CA 217

5.7.4E TX–RX frequency separation for category M1 and M2 217

5.7.4F TX–RX frequency separation for category NB1 and NB2 218

6 Transmitter characteristics 218

6.1 General 218

6.2 Transmit power 218

6.2.1 Void 218

6.2.2 UE maximum output power 218

6.2.2A UE maximum output power for CA 221

6.2.2B UE maximum output power for UL-MIMO 226

6.2.2C Void 229

6.2.2D UE maximum output power for ProSe 229

6.2.2E UE maximum output power for Category M1 and M2 UE 229

6.2.2F UE maximum output power for category NB1 and NB2 230

6.2.2G UE maximum output power for V2X Communication 231

6.2.2K UE maximum output power for Aerial UE 233

6.2.3 UE maximum output power for modulation / channel bandwidth 233

6.2.3A UE Maximum Output power for modulation / channel bandwidth for CA 234

6.2.3B UE maximum output power for modulation / channel bandwidth for UL-MIMO 239

6.2.3D UE maximum output power for modulation / channel bandwidth for ProSe 239

6.2.3E UE maximum output power for modulation / channel bandwidth for category M1 and M2 240

6.2.3F UE maximum output power for modulation / channel bandwidth for category NB1 and NB2 242

6.2.3G UE maximum output power for modulation / channel bandwidth for V2X Communication 243

6.2.3G.1 MPR for Power class 3 V2X UE 243

6.2.3G.2 MPR for Power class 2 V2X UE 244

6.2.3K UE maximum output power for modulation / channel bandwidth for Aerial UE 245

6.2.4 UE maximum output power with additional requirements 245

6.2.4A UE maximum output power with additional requirements for CA 265

6.2.4A.1 A-MPR for CA\_NS\_01 for CA\_1C 267

6.2.4A.2 A-MPR for CA\_NS\_02 for CA\_1C 268

6.2.4A.3 A-MPR for CA\_NS\_03 for CA\_1C 269

6.2.4A.4 A-MPR for CA\_NS\_04 270

6.2.4A.5 A-MPR for CA\_NS\_05 for CA\_38C 272

6.2.4A.6 A-MPR for CA\_NS\_06 273

6.2.4A.7 A-MPR for CA\_NS\_07 274

6.2.4A.8 A-MPR for CA\_NS\_08 275

6.2.4A.9 Void 276

6.2.4A.10 A-MPR for CA\_NS\_10 276

6.2.4A.11 A-MPR for CA\_NS\_11 281

6.2.4A.12 A-MPR for CA\_NS\_12 281

6.2.4A.13 A-MPR for CA\_NS\_13 282

6.2.4A.14 A-MPR for CA\_NS\_17 283

6.2.4A.15 A-MPR for CA\_NS\_18 284

6.2.4B UE maximum output power with additional requirements for UL-MIMO 286

6.2.4D UE maximum output power with additional requirements for ProSe 286

6.2.4E UE maximum output power with additional requirements for category M1 and M2 UE 286

6.2.4F UE maximum output power with additional requirements for category NB1 and NB2 UE 297

6.2.4G UE maximum output power with additional requirements for V2X Communication 297

6.2.5 Configured transmitted power 300

6.2.5A Configured transmitted power for CA 336

6.2.5B Configured transmitted power for UL-MIMO 340

6.2.5C Configured transmitted power for Dual Connectivity 341

6.2.5D Configured transmitted power for ProSe 342

6.2.5F Configured transmitted Power for category NB1 and NB2 344

6.2.5G Configured transmitted power for V2X Communication 345

6.2.5K Configured transmitted power for Aerial UE 349

6.3 Output power dynamics 349

6.3.1 (Void) 349

6.3.2 Minimum output power 349

6.3.2.1 Minimum requirement 349

6.3.2A UE Minimum output power for CA 349

6.3.2A.1 Minimum requirement for CA 349

6.3.2B UE Minimum output power for UL-MIMO 350

6.3.2B.1 Minimum requirement 350

6.3.2C Void 350

6.3.2D UE Minimum output power for ProSe 350

6.3.2F UE Minimum output power for category NB1 and NB2 350

6.3.2G UE Minimum output power for V2X Communication 351

6.3.3 Transmit OFF power 351

6.3.3.1. Minimum requirement 351

6.3.3A UE Transmit OFF power for CA 351

6.3.3A.1 Minimum requirement for CA 352

6.3.3B UE Transmit OFF power for UL-MIMO 352

6.3.3B.1 Minimum requirement 352

6.3.3D Transmit OFF power for ProSe 352

6.3.3F Transmit OFF power for category NB1 and NB2 353

6.3.3G Transmit OFF power for V2X Communication 353

6.3.4 ON/OFF time mask 353

6.3.4.1 General ON/OFF time mask 353

6.3.4.2 PRACH and SRS time mask 355

6.3.4.2.1 PRACH time mask 355

6.3.4.2.2 SRS time mask 355

6.3.4.3 Slot / Sub frame boundary time mask for subframe TTI 357

6.3.4.4 PUCCH / PUSCH / SRS time mask for subframe TTI 359

6.3.4.5 Symbol / Subslot boundary time mask for subslot TTI 361

6.3.4.6 Subslot PUCCH / subslot PUSCH / SRS time mask for subslot TTI 363

6.3.4.7 Symbol / Slot boundary time mask for slot TTI 366

6.3.4.8 Slot PUCCH / slot PUSCH / SRS time mask for slot TTI 366

6.3.4.9 Consecutive subslot and slot TTI or consecutive subslot and subframe TTI time mask 367

6.3.4.10 Consecutive subframe and subslot TTI or consecutive slot and subslot TTI time mask 367

6.3.4.11 Consecutive TTI and slot TTI or consecutive slot TTI and TTI time mask 368

6.3.4A ON/OFF time mask for CA 368

6.3.4B ON/OFF time mask for UL-MIMO 368

6.3.4D ON/OFF time mask for ProSe 369

6.3.4D.1 General time mask for ProSe 369

6.3.4D.2 PSSS/SSSS time mask 369

6.3.4D.3 PSSS / SSSS / PSBCH time mask 370

6.3.4D.4 PSSCH / SRS time mask 371

6.3.4F ON/OFF time mask for category NB1 and NB2 371

6.3.4F.1 General ON/OFF time mask 371

6.3.4F.2 NPRACH time mask 371

6.3.4G ON/OFF time mask for V2X Communication 372

6.3.4G.1 PSSS / SSSS / PSBCH time mask 372

6.3.5 Power Control 373

6.3.5.1 Absolute power tolerance 373

6.3.5.1.1 Minimum requirements 373

6.3.5.2 Relative Power tolerance 374

6.3.5.2.1 Minimum requirements 374

6.3.5.3 Aggregate power control tolerance 375

6.3.5.3.1 Minimum requirement 375

6.3.5A Power control for CA 375

6.3.5A.1 Absolute power tolerance 375

6.3.5A.1.1 Minimum requirements 375

6.3.5A.2 Relative power tolerance 376

6.3.5A.2.1 Minimum requirements 376

6.3.5A.3 Aggregate power control tolerance 376

6.3.5A.3.1 Minimum requirements 376

6.3.5B Power control for UL-MIMO 377

6.3.5D Power Control for ProSe 377

6.3.5D.1 Absolute power tolerance 377

6.3.5E Power control for category M1 and M2 377

6.3.5E.1 Absolute power tolerance 377

6.3.5E.2 Relative Power tolerance 377

6.3.5E.3 Aggregate power control tolerance 378

6.3.5E.3.1 Minimum requirement 378

6.3.5F Power Control for category NB1 and NB2 378

6.3.5F.1 Absolute power tolerance 379

6.3.5F.2 Relative power tolerance 379

6.3.5F.3 Aggregate power control tolerance for category NB1 and NB2 380

6.3.5F.3.1 Minimum requirement 380

6.3.5G Power Control for V2X Communication 380

6.3.5G.1 Absolute power tolerance 380

6.4 Void 381

6.5 Transmit signal quality 381

6.5.1 Frequency error 381

6.5.1A Frequency error for CA 381

6.5.1B Frequency error for UL-MIMO 381

6.5.1D Frequency error for ProSe 381

6.5.1E Frequency error for UE category M1 and M2 381

6.5.1F Frequency error for UE category NB1 and NB2 382

6.5.1G Frequency error for V2X Communication 382

6.5.2 Transmit modulation quality 382

6.5.2.1 Error Vector Magnitude 383

6.5.2.1.1 Minimum requirement 383

6.5.2.2 Carrier leakage 383

6.5.2.2.1 Minimum requirements 384

6.5.2.3 In-band emissions 384

6.5.2.3.1 Minimum requirements 384

6.5.2.4 EVM equalizer spectrum flatness 385

6.5.2.4.1 Minimum requirements 385

6.5.2A Transmit modulation quality for CA 386

6.5.2A.1 Error Vector Magnitude 387

6.5.2A.2 Carrier leakage for CA 387

6.5.2A.2.1 Minimum requirements 387

6.5.2A.3 In-band emissions 387

6.5.2A.3.1 Minimum requirement for CA 387

6.5.2B Transmit modulation quality for UL-MIMO 390

6.5.2B.1 Error Vector Magnitude 390

6.5.2B.2 Carrier leakage 390

6.5.2B.3 In-band emissions 390

6.5.2B.4 EVM equalizer spectrum flatness for UL-MIMO 390

6.5.2D Transmit modulation quality for ProSe 390

6.5.2D.1 Error Vector Magnitude 390

6.5.2D.2 Carrier leakage 391

6.5.2D.3 In-band emissions 391

6.5.2D.4 EVM equalizer spectrum flatness for ProSe 391

6.5.2E Transmit modulation quality for category M1 and M2 391

6.5.2E.1 Error Vector Magnitude 391

6.5.2E.2 Carrier leakage 391

6.5.2E.2.1 Minimum requirements 391

6.5.2E.3 In-band emissions 391

6.5.2E.3.1 Minimum requirements 391

6.5.2F Transmit modulation quality for Category NB1 and NB2 393

6.5.2F.1 Error Vector Magnitude 393

6.5.2F.2 Carrier leakage 393

6.5.2F.3 In-band emissions 393

6.5.2G Transmit modulation quality for V2X Communication 394

6.5.2G.1 Error Vector Magnitude 394

6.5.2G.2 Carrier leakage 395

6.5.2G.3 In-band emissions 395

6.5.2G.4 EVM equalizer spectrum flatness 395

6.6 Output RF spectrum emissions 395

6.6.1 Occupied bandwidth 395

6.6.1.1 Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 396

6.6.1A Occupied bandwidth for CA 396

6.6.1B Occupied bandwidth for UL-MIMO 396

6.6.1F Occupied bandwidth for category NB1 and NB2 397

6.6.1G Occupied bandwidth for V2X Communication 397

6.6.2 Out of band emission 397

6.6.2.1 Spectrum emission mask 397

6.6.2.1.1 Minimum requirement 397

6.6.2.1A Spectrum emission mask for CA 398

6.6.2.2 Additional spectrum emission mask 399

6.6.2.2.1 Minimum requirement (network signalled value "NS\_03", “NS\_11”, "NS\_20", and “NS\_21”) 399

6.6.2.2.2 Minimum requirement (network signalled value "NS\_04") 400

6.6.2.2.3 Minimum requirement (network signalled value "NS\_06" or “NS\_07”) 400

6.6.2.2.4 Minimum requirement (network signalled value "NS\_33" or “NS\_34”) 401

6.6.2.2.5 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 401

6.6.2.2.6 Minimum requirement (network signalled value "NS\_28”) 402

6.6.2.2.7 Minimum requirement (network signalled value "NS\_35") 402

6.6.2.2A Additional Spectrum Emission Mask for CA 403

6.6.2.2A.1 Minimum requirement (network signalled value "CA\_NS\_04") 403

6.6.2.2A.2 Minimum requirement CA\_66B (network signalled value "CA\_NS\_09") 403

6.6.2.2A.3 Minimum requirement CA\_66C (network signalled value "CA\_NS\_09") 404

6.6.2.2A.4 Minimum requirement CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 404

6.6.2.2A.5 Minimum requirement CA\_2C (network signalled value "CA\_NS\_11") 405

6.6.2.3 Adjacent Channel Leakage Ratio 406

6.6.2.3.1 Minimum requirement E-UTRA 407

6.6.2.3.1a Additional minimum requirement for E-UTRA (network signalled value “NS\_29”) 408

6.6.2.3.1A Void 408

6.6.2.3.1Aa Void 408

6.6.2.3.2 Minimum requirements UTRA 408

6.6.2.3.2A Minimum requirement UTRA for CA 409

6.6.2.3.3A Minimum requirements for CA E-UTRA 411

6.6.2.4 Void 412

6.6.2.4.1 Void 412

6.6.2A Void 412

6.6.2B Out of band emission for UL-MIMO 412

6.6.2C Void 412

6.6.2D Out of band emission for ProSe 413

6.6.2F Out of band emission for category NB1 and NB2 413

6.6.2F.1 Spectrum emission mask 413

6.6.2F.2 Additional Spectrum Emission Mask for Category NB1 and NB2 413

6.6.2F.2.1 Minimum requirement (network signalled value "NS\_02") 413

6.6.2F.2.2 Minimum requirement (network signalled value "NS\_03") 414

6.6.2F.3 Adjacent Channel Leakage Ratio for category NB1 and NB2 414

6.6.2G Out of band emission for V2X Communication 414

6.6.3 Spurious emissions 415

6.6.3.1 Minimum requirements 415

6.6.3.1A Minimum requirements for CA 416

6.6.3.2 Spurious emission band UE co-existence 417

6.6.3.2A Spurious emission band UE co-existence for CA 427

6.6.3.3 Additional spurious emissions 437

6.6.3.3.1 Minimum requirement (network signalled value "NS\_05") 437

6.6.3.3.2 Minimum requirement (network signalled value “NS\_07”) 437

6.6.3.3.3 Minimum requirement (network signalled value “NS\_08”) 437

6.6.3.3.4 Minimum requirement (network signalled value “NS\_09”) 438

6.6.3.3.5 Minimum requirement (network signalled value "NS\_12") 438

6.6.3.3.6 Minimum requirement (network signalled value “NS\_13”) 438

6.6.3.3.7 Minimum requirement (network signalled value “NS\_14”) 438

6.6.3.3.8 Minimum requirement (network signalled value “NS\_15”) 439

6.6.3.3.9 Minimum requirement (network signalled value “NS\_16”) 439

6.6.3.3.10 Minimum requirement (network signalled value “NS\_17”) 439

6.6.3.3.11 Minimum requirement (network signalled value “NS\_18”) 440

6.6.3.3.12 Minimum requirement (network signalled value “NS\_19”) 440

6.6.3.3.13 Minimum requirement (network signalled value “NS\_11”) 440

6.6.3.3.14 Minimum requirement (network signalled value “NS\_20”) 440

6.6.3.3.15 Minimum requirement (network signalled value “NS\_21”) 441

6.6.3.3.16 Minimum requirement (network signalled value "NS\_22") 441

6.6.3.3.17 Minimum requirement (network signalled value “NS\_23”) 441

6.6.3.3.18 Void 442

6.6.3.3.19 Minimum requirement (network signalled value "NS\_04") 442

6.6.3.3.20 Minimum requirement (network signalled value “NS\_24”) 442

6.6.3.3.21 Minimum requirement (network signalled value “NS\_25”) 443

6.6.3.3.22 Minimum requirement (network signalled value “NS\_26”) 443

6.6.3.3.23 Minimum requirement (network signalled value “NS\_27” and “NS\_43”) 443

6.6.3.3.24 Minimum requirement (network signalled value “NS\_28”) 443

6.6.3.3.25 Minimum requirement (network signalled value “NS\_29”) 444

6.6.3.3.26 Minimum requirement (network signalled value “NS\_30”) 444

6.6.3.3.27 Minimum requirement (network signalled value “NS\_31”) 445

6.6.3.3.28 Minimum requirement (network signalled value “NS\_36”) 446

6.6.3.3.29 Minimum requirement (network signalled value “NS\_38”) 446

6.6.3.3.30 Minimum requirement (network signalled value “NS\_39”) 446

6.6.3.3.31 Minimum requirement (network signalled value “NS\_40” and “NS\_41”) 447

6.6.3.3.32 Minimum requirement (network signalled value “NS\_42”) 447

6.6.3.3.33 Minimum requirement (network signalled value “NS\_44”) 447

6.6.3.3.34 Minimum requirement (network signalled value “NS\_45”) 447

6.6.3.3.35 Minimum requirement (network signalled value “NS\_56”) 448

6.6.3.3.36 Minimum requirement (network signalled value “NS\_62”) 448

6.6.3.3A Additional spurious emissions for CA 449

6.6.3.3A.1 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_01") 449

6.6.3.3A.2 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_02") 449

6.6.3.3A.3 Minimum requirement for CA\_1C (network signalled value "CA\_NS\_03") 450

6.6.3.3A.4 Minimum requirement for CA\_38C (network signalled value "CA\_NS\_05") 450

6.6.3.3A.5 Minimum requirement for CA\_7C (network signalled value "CA\_NS\_06") 450

6.6.3.3A.6 Minimum requirement for CA\_39C and CA\_39C-41A (network signalled value "CA\_NS\_07") 451

6.6.3.3A.7 Minimum requirement for CA\_42C (network signalled value "CA\_NS\_08") 451

6.6.3.3A.8 Minimum requirement for CA\_41C and CA\_41D (network signalled value "CA\_NS\_04") 451

6.6.3.3A.9 Void 452

6.6.3.3A.10 Minimum requirement for CA\_48B and CA\_48C (network signalled value "CA\_NS\_10") 452

6.6.3.3A.11 Minimum requirement for CA\_28C (network signalled value "CA\_NS\_12") 452

6.6.3.3A.12 Minimum requirement for CA\_28C (network signalled value "CA\_NS\_13") 452

6.6.3A Void 453

6.6.3B Spurious emission for UL-MIMO 453

6.6.3C Void 453

6.6.3D Spurious emission for ProSe 453

6.6.3F Spurious emission for category NB1 and NB2 453

6.6.3F.1 Additional spurious emissions 453

6.6.3F.1.2 Minimum requirement (network signalled value "NS\_06") 453

6.6.3G Spurious emission for V2X Communication 454

6.6.3K Spurious emission for Aerial UE 456

6.6A Void 457

6.6B Void 457

6.7 Transmit intermodulation 457

6.7.1 Minimum requirement 457

6.7.1A Minimum requirement for CA 457

6.7.1B Minimum requirement for UL-MIMO 458

6.7.1F Minimum requirement for category NB1 and NB2 458

6.7.1G Minimum requirement for V2X Communication 458

6.8 Void 459

6.8A Void 459

6.8B Time alignment error for UL-MIMO 459

6.8B.1 Minimum Requirements 459

6.8C Void 459

6.8D Void 459

6.8E Void 459

6.8F Void 459

6.8G Time alignment error 459

7 Receiver characteristics 459

7.1 General 459

7.2 Diversity characteristics 460

7.3 Reference sensitivity power level 460

7.3.1 Minimum requirements (QPSK) 461

7.3.1A Minimum requirements (QPSK) for CA 501

7.3.1B Minimum requirements (QPSK) for UL-MIMO 549

7.3.1D Minimum requirements (QPSK) for ProSe 549

7.3.1E Minimum requirements (QPSK) for UE category 0, M1, M2 and 1bis 551

7.3.1F Minimum requirements for UE category NB1 and NB2 563

7.3.1F.1 Reference sensitivity for UE category NB1 and NB2 563

7.3.1F.2 Void 564

7.3.1G Minimum requirements (QPSK) for V2X 564

7.3.1H Minimum requirements for LTE based 5G terrestrial broadcast 566

7.3.2 Void 567

7.4 Maximum input level 567

7.4.1 Minimum requirements 567

7.4.1A Minimum requirements for CA 567

7.4.1B Minimum requirements for UL-MIMO 569

7.4.1D Minimum requirements for ProSe 569

7.4.1F Minimum requirements for category NB1 and NB2 569

7.4.1G Minimum requirements for V2X 569

7.4.1H Minimum requirements for LTE based 5G terrestrial broadcast 570

7.4A Void 570

7.4A.1 Void 570

7.5 Adjacent Channel Selectivity (ACS) 570

7.5.1 Minimum requirements 570

7.5.1A Minimum requirements for CA 571

7.5.1B Minimum requirements for UL-MIMO 576

7.5.1D Minimum requirements for ProSe 576

7.5.1F Minimum requirements for category NB1 and NB2 576

7.5.1G Minimum requirements for V2X 577

7.5.1H Minimum requirements for LTE based 5G terrestrial broadcast 579

7.6 Blocking characteristics 580

7.6.1 In-band blocking 580

7.6.1.1 Minimum requirements 580

7.6.1.1A Minimum requirements for CA 582

7.6.1.1D Minimum requirements for ProSe 585

7.6.1.1F Minimum requirements for category NB1 and NB2 586

7.6.1.1G Minimum requirements for V2X 586

7.6.1.1H Minimum requirements for LTE based 5G terrestrial broadcast 588

7.6.2 Out-of-band blocking 589

7.6.2.1 Minimum requirements 589

7.6.2.1A Minimum requirements for CA 590

7.6.2.1D Minimum requirements for ProSe 594

7.6.2.1F Minimum requirements for category NB1 and NB2 594

7.6.2.1G Minimum requirements for V2X 595

7.6.2.1H Minimum requirements for LTE based 5G terrestrial broadcast 596

7.6.3 Narrow band blocking 597

7.6.3.1 Minimum requirements 597

7.6.3.1A Minimum requirements for CA 598

7.6.3.1D Minimum requirements for ProSe 599

7.6.3.1H Minimum requirements for LTE based 5G terrestrial broadcast 599

7.6A Void 599

7.6B Blocking characteristics for UL-MIMO 599

7.7 Spurious response 600

7.7.1 Minimum requirements 600

7.7.1A Minimum requirements for CA 600

7.7.1B Minimum requirements for UL-MIMO 601

7.7.1D Minimum requirements for ProSe 601

7.7.1F Minimum requirements for UE category NB1 and NB2 602

7.7.1G Minimum requirements for V2X 602

7.7.1H Minimum requirements for LTE based 5G terrestrial broadcast 603

7.8 Intermodulation characteristics 604

7.8.1 Wide band intermodulation 604

7.8.1.1 Minimum requirements 604

7.8.1A Minimum requirements for CA 605

7.8.1B Minimum requirements for UL-MIMO 608

7.8.1D Minimum requirements for ProSe 608

7.8.1F Minimum requirements for category NB1 and NB2 609

7.8.1G Minimum requirements 609

7.8.1H Minimum requirements for LTE based 5G terrestrial broadcast 610

7.8.2 Void 611

7.9 Spurious emissions 611

7.9.1 Minimum requirements 611

7.9.1A Minimum requirements 612

7.10 Receiver image 612

7.10.1 Void 612

7.10.1A Minimum requirements for CA 612

7.10.1G Minimum requirements for V2X Communication 612

8 Performance requirement 643

8.1 General 643

8.1.1 Receiver antenna capability 643

8.1.1.1 Simultaneous unicast and MBMS operations 644

8.1.1.2 Dual-antenna receiver capability in idle mode 644

8.1.2 Applicability of requirements 644

8.1.2.1 Applicability of requirements for different channel bandwidths 644

8.1.2.2 Definition of CA capability 644

8.1.2.2A Definition of dual connectivity capability 649

8.1.2.3 Applicability and test rules for different CA configurations and bandwidth combination sets 650

8.1.2.3A Applicability and test rules for different dual connectivity configuration and bandwidth combination set 653

8.1.2.3B Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 654

8.1.2.3C Applicability and test rules for SDR tests for 4Rx capable UEs 656

8.1.2.3D Applicability and test rules for different CA with LAA SCell(s) configurations and bandwidth combination sets 656

8.1.2.3E Applicability and test rules for SDR tests for 8Rx capable UEs 657

8.1.2.4 Test coverage for different number of component carriers 658

8.1.2.5 Applicability of performance requirements for Type B receiver 659

8.1.2.6 Applicability of performance requirements for 4Rx capable UEs 659

8.1.2.6.1 Applicability rule and antenna connection for single carrier tests with 2Rx 659

8.1.2.6.2 Applicability rule and antenna connection for CA and DC tests with 2Rx 661

8.1.2.6.3 Applicability rule and antenna connection for single carrier tests with 4Rx 661

8.1.2.6.4 Applicability rule for 256QAM tests 662

8.1.2.6.5 Applicability rule and antenna connection for CA and DC tests with 4Rx 662

8.1.2.6.6 Applicability rule for Type C with 4Rx 666

8.1.2.6.7 Applicability rule for 1024QAM tests 666

8.1.2.7 Applicability of Enhanced Downlink Control Channel Performance Requirements 666

8.1.2.8 Applicability of performance requirements for CDM-multiplexed DM RS with interfering simultaneous transmission (FRC) with multiple CSI-RS configurations 668

8.1.2.8A Applicability of performance requirements for UE supporting coverage enhancement 668

8.1.2.9 Applicability of SDR requirements for CA and LAA 669

8.1.2.10 Applicability of performance requirements for Multi-user Superposed Transmission 670

8.1.2.11 Applicability CRS interference mitigation receivers performance requirements 670

8.1.2.12 Applicability of performance requirements for 8Rx capable UEs 671

8.1.2.12.1 Applicability rule and antenna connection for single carrier PDSCH tests 671

8.1.2.12.2 Applicability rule and antenna connection for control channel tests 677

8.1.2.12.3 Applicability rule and antenna connection for CA and DC tests 677

8.1.3 UE category and UE DL category 678

8.2 Demodulation of PDSCH (Cell-Specific Reference Symbols) 678

8.2.1 FDD (Fixed Reference Channel) 678

8.2.1.1 Single-antenna port performance 679

8.2.1.1.1 Minimum Requirement 679

8.2.1.1.2 Void 685

8.2.1.1.3 Void 685

8.2.1.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 685

8.2.1.1.4A Minimum Requirement 1 PRB allocation in presence of FeMBMS Unicast-mixed Cell under CA 685

8.2.1.2 Transmit diversity performance 686

8.2.1.2.1 Minimum Requirement 2 Tx Antenna Port 686

8.2.1.2.2 Minimum Requirement 4 Tx Antenna Port 687

8.2.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 687

8.2.1.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 689

8.2.1.2.4 Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 691

8.2.1.2.5 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 693

8.2.1.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 694

8.2.1.2.7 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 695

8.2.1.3 Open-loop spatial multiplexing performance 695

8.2.1.3.1 Minimum Requirement 2 Tx Antenna Port 695

8.2.1.3.1A Soft buffer management test 699

8.2.1.3.1B Enhanced Performance Requirement Type C –2Tx Antenna Ports 700

8.2.1.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 701

8.2.1.3.2 Minimum Requirement 4 Tx Antenna Port 702

8.2.1.3.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 702

8.2.1.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 706

8.2.1.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 708

8.2.1.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 709

8.2.1.4 Closed-loop spatial multiplexing performance 710

8.2.1.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 710

8.2.1.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 711

8.2.1.4.1B Enhanced Performance Requirement Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 711

8.2.1.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 713

8.2.1.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 716

8.2.1.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 718

8.2.1.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 719

8.2.1.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 720

8.2.1.4.2A Enhanced Performance Requirement Type C – Multi-layer Spatial Multiplexing 2Tx Antenna Ports 721

8.2.1.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 721

8.2.1.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 725

8.2.1.4.4 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 727

8.2.1.5 MU-MIMO 728

8.2.1.6 [Control channel performance: D-BCH and PCH] 728

8.2.1.7 Carrier aggregation with power imbalance 728

8.2.1.7.1 Minimum Requirement 728

8.2.1.8 Intra-band non-contiguous carrier aggregation with timing offset 729

8.2.1.8.1 Minimum Requirement 729

8.2.1.9 HST-SFN performance 730

8.2.1.9.1 Minimum Requirement 730

8.2.1.9.2 Minimum Requirement for Rel-16 further enhanced HST 733

8.2.1.10 Intra-band contiguous carrier aggregation with minimum channel spacing 733

8.2.1.10.1 Minimum Requirement 734

8.2.2 TDD (Fixed Reference Channel) 734

8.2.2.1 Single-antenna port performance 735

8.2.2.1.1 Minimum Requirement 735

8.2.2.1.2 Void 740

8.2.2.1.3 Void 740

8.2.2.1.4 Minimum Requirement 1 PRB allocation in presence of MBSFN 740

8.2.2.2 Transmit diversity performance 740

8.2.2.2.1 Minimum Requirement 2 Tx Antenna Port 740

8.2.2.2.2 Minimum Requirement 4 Tx Antenna Port 741

8.2.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 742

8.2.2.2.3A Minimum Requirement 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 743

8.2.2.2.4 Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 745

8.2.2.2.5 Minimum Requirement 2 Tx Antenna Port (when *EIMTA-MainConfigServCell-r12* is configured) 747

8.2.2.2.6 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM2 interference model 747

8.2.2.2.7 Enhanced Performance Requirement Type B - 2 Tx Antenna Ports with TM9 interference model 749

8.2.2.2.8 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 750

8.2.2.3 Open-loop spatial multiplexing performance 751

8.2.2.3.1 Minimum Requirement 2 Tx Antenna Port 751

8.2.2.3.1A Soft buffer management test 754

8.2.2.3.1B Enhanced Performance Requirement Type C - 2Tx Antenna Ports 754

8.2.2.3.1C Enhanced Performance Requirement Type C - 2 Tx Antenna Ports with TM1 interference 755

8.2.2.3.2 Minimum Requirement 4 Tx Antenna Port 756

8.2.2.3.3 Minimum Requirement 2Tx antenna port (demodulation subframe overlaps with aggressor cell ABS) 757

8.2.2.3.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 761

8.2.2.3.5 Minimum Requirement 2 Tx Antenna Port (Superposed transmission) 763

8.2.2.3.6 Minimum Requirement 2 Tx Antenna Port (network-based CRS interference mitigation) 764

8.2.2.4 Closed-loop spatial multiplexing performance 765

8.2.2.4.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port 765

8.2.2.4.1A Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Port 766

8.2.2.4.1B Enhanced Performance Requirement Type A – Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 766

8.2.2.4.1C Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 768

8.2.2.4.1D Enhanced Performance Requirement Type B - Single-layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model 770

8.2.2.4.1E Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Ports with CRS assistance information 772

8.2.2.4.1F Minimum Requirement Single-Layer Spatial Multiplexing 4 Tx Antenna Ports with CRS assistance information 773

8.2.2.4.2 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 775

8.2.2.4.2A Enhanced Performance Requirement Type C Multi-Layer Spatial Multiplexing 2 Tx Antenna Port 775

8.2.2.4.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 776

8.2.2.4.3A Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 780

8.2.2.4.4 Void 781

8.2.2.4.5 Minimum Requirement Multi-Layer Spatial Multiplexing 2 Tx Antenna Port (Superposed transmission) 781

8.2.2.5 MU-MIMO 782

8.2.2.6 [Control channel performance: D-BCH and PCH] 782

8.2.2.7 Carrier aggregation with power imbalance 782

8.2.2.7.1 Minimum Requirement 782

8.2.2.8 Intra-band contiguous carrier aggregation with minimum channel spacing 783

8.2.2.8.1 Minimum Requirement 783

8.2.2.9 HST-SFN performance 784

8.2.2.9.1 Minimum Requirement 784

8.2.2.9.2 Minimum Requirement for Rel-16 further enhanced HST 786

8.2.3 TDD FDD CA (Fixed Reference Channel) 787

8.2.3.1 Single-antenna port performance 788

8.2.3.1.1 Minimum Requirement for FDD PCell 788

8.2.3.1.2 Minimum Requirement for TDD PCell 792

8.2.3.2 Open-loop spatial multiplexing performance 2Tx Antenna port 796

8.2.3.2.1 Minimum Requirement for FDD PCell 796

8.2.3.2.1A Soft buffer management test for FDD PCell 800

8.2.3.2.2 Minimum Requirement for TDD PCell 801

8.2.3.2.2A Soft buffer management test for TDD PCell 805

8.2.3.3 Closed-loop spatial multiplexing performance 4Tx Antenna Port 806

8.2.3.3.1 Minimum Requirement for FDD PCell 806

8.2.3.3.2 Minimum Requirement for TDD PCell 810

8.2.3.4 Minimum Requirement for Closed-loop spatial multiplexing performance 4Tx Antenna Port for dual connectivity 814

8.2.3.5 HST-SFN performance 816

8.2.3.5.0 General 816

8.2.3.5.1 Minimum Requirement for FDD PCell 816

8.2.3.5.2 Minimum Requirement for TDD PCell 819

8.2.4 LAA 822

8.2.4.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 822

8.2.4.1.1 FDD PCell (FDD single carrier) 822

8.2.4.1.2 TDD PCell (TDD single carrier) 826

8.3 Demodulation of PDSCH (User-Specific Reference Symbols) 829

8.3.1 FDD 829

8.3.1.1 Single-layer Spatial Multiplexing 830

8.3.1.1A Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 832

8.3.1.1B Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 835

8.3.1.1C Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference model 838

8.3.1.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 840

8.3.1.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference model 841

8.3.1.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 842

8.3.1.1G Single-layer Spatial Multiplexing (CRS assistance information is configured) 844

8.3.1.1H Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 846

8.3.1.1I Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 847

8.3.1.2 Dual-Layer Spatial Multiplexing 849

8.3.1.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 850

8.3.1.3 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 851

8.3.1.3.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 851

8.3.1.3.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 853

8.3.1.3.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 855

8.3.1.3.4 Minimum requirement with Different Cell ID and non-colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 857

8.3.1.3.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 859

8.3.1.3.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 862

8.3.1.4 Performance Requirements for semiOpenLoop transmission 864

8.3.2 TDD 866

8.3.2.1 Single-layer Spatial Multiplexing 866

8.3.2.1A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 868

8.3.2.1B Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model 870

8.3.2.1C Single-layer Spatial Multiplexing (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 873

8.3.2.1D Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM9 interference 876

8.3.2.1E Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with CRS interference model 878

8.3.2.1F Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM3 interference 880

8.3.2.1G Enhanced Performance Requirement Type B – Single-layer Spatial Multiplexing with TM10 serving cell configuration and TM9 interference model 881

8.3.2.1H Single-layer Spatial Multiplexing (CRS assistance information is configured) 883

8.3.2.1I Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 885

8.3.2.1J Single-layer Spatial Multiplexing (with assistance information for simultaneous transmition interfering PDSCH) 886

8.3.2.2 Dual-Layer Spatial Multiplexing 888

8.3.2.2A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 888

8.3.2.3 Dual-Layer Spatial Multiplexing (with multiple CSI-RS configurations) 889

8.3.2.4 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 890

8.3.2.4.1 Minimum requirement with Same Cell ID (with single NZP CSI-RS resource) 890

8.3.2.4.2 Minimum requirements with Same Cell ID (with multiple NZP CSI-RS resources) 892

8.3.2.4.3 Minimum requirement with Different Cell ID and Colliding CRS (with single NZP CSI-RS resource) 894

8.3.2.4.4 Minimum requirement with Different Cell ID and non-Colliding CRS (with single NZP CSI-RS resource and CRS assistance information is configured) 896

8.3.2.4.5 Minimum requirements with different Cell ID and non-colliding CRS (with multiple NZP CSI-RS resources and CRS assistance information is configured) 898

8.3.2.4.6 Minimum requirements for QCL Type C and 2 Layers Spatial Multiplexing 901

8.3.2.5 Performance Requirements for semiOpenLoop transmission 903

8.3.3 LAA 905

8.3.3.1 Dual-Layer Spatial Multiplexing with DM-RS 905

8.3.3.1.1 FDD PCell (FDD single carrier) 905

8.3.3.1.2 TDD Pcell (TDD single carrier) 910

8.4 Demodulation of PDCCH/PCFICH 914

8.4.1 FDD 914

8.4.1.1 Single-antenna port performance 915

8.4.1.2 Transmit diversity performance 915

8.4.1.2.1 Minimum Requirement 2 Tx Antenna Port 915

8.4.1.2.2 Minimum Requirement 4 Tx Antenna Port 915

8.4.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 916

8.4.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 921

8.4.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port under Asynchronous Network 927

8.4.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 928

8.4.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 929

8.4.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 930

8.4.1.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 931

8.4.2 TDD 932

8.4.2.1 Single-antenna port performance 933

8.4.2.2 Transmit diversity performance 933

8.4.2.2.1 Minimum Requirement 2 Tx Antenna Port 933

8.4.2.2.2 Minimum Requirement 4 Tx Antenna Port 934

8.4.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 934

8.4.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 938

8.4.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 942

8.4.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 943

8.4.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Colliding CRS Dominant Interferer 944

8.4.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 945

8.4.2.2.9 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 946

8.4.3 LAA 947

8.4.3.1 Transmit diversity performance 947

8.4.3.1.1 FDD Pcell (FDD single carrier) 947

8.4.3.1.2 TDD Pcell (TDD single carrier) 948

8.5 Demodulation of PHICH 949

8.5.1 FDD 950

8.5.1.1 Single-antenna port performance 950

8.5.1.2 Transmit diversity performance 950

8.5.1.2.1 Minimum Requirement 2 Tx Antenna Port 950

8.5.1.2.2 Minimum Requirement 4 Tx Antenna Port 951

8.5.1.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 951

8.5.1.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 953

8.5.1.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports under Asynchronous Network 956

8.5.1.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 957

8.5.1.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 958

8.5.1.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 959

8.5.2 TDD 960

8.5.2.1 Single-antenna port performance 961

8.5.2.2 Transmit diversity performance 961

8.5.2.2.1 Minimum Requirement 2 Tx Antenna Port 961

8.5.2.2.2 Minimum Requirement 4 Tx Antenna Port 962

8.5.2.2.3 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS) 962

8.5.2.2.4 Minimum Requirement 2 Tx Antenna Port (demodulation subframe overlaps with aggressor cell ABS and CRS assistance information are configured) 964

8.5.2.2.5 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 966

8.5.2.2.6 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 967

8.5.2.2.7 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Colliding CRS Dominant Interferer 968

8.5.2.2.8 Enhanced Downlink Control Channel Performance Requirement Type B - 2 Tx Antenna Ports with Non-Colliding CRS Dominant Interferer 969

8.6 Demodulation of PBCH 970

8.6.1 FDD 970

8.6.1.1 Single-antenna port performance 970

8.6.1.2 Transmit diversity performance 971

8.6.1.2.1 Minimum Requirement 2 Tx Antenna Port 971

8.6.1.2.2 Minimum Requirement 4 Tx Antenna Port 971

8.6.1.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 971

8.6.2 TDD 973

8.6.2.1 Single-antenna port performance 973

8.6.2.2 Transmit diversity performance 973

8.6.2.2.1 Minimum Requirement 2 Tx Antenna Port 973

8.6.2.2.2 Minimum Requirement 4 Tx Antenna Port 973

8.6.2.2.3 Minimum Requirement 2 Tx Antenna Port under Time Domain Measurement Resource Restriction with CRS Assistance Information 974

8.7 Sustained downlink data rate provided by lower layers 975

8.7.1 FDD (single carrier and CA) 975

8.7.2 TDD (single carrier and CA) 992

8.7.3 FDD (EPDCCH scheduling) 996

8.7.4 TDD (EPDCCH scheduling) 998

8.7.5 TDD FDD CA 1000

8.7.5.1 Minimum Requirement FDD PCell 1001

8.7.5.2 Minimum Requirement TDD PCell 1009

8.7.6 FDD (DC) 1018

8.7.7 TDD (DC) 1025

8.7.8 TDD FDD (DC) 1028

8.7.9 FDD (4 Rx) 1031

8.7.10 TDD (4 Rx) 1033

8.7.11 TDD FDD CA (4 Rx) 1035

8.7.11.1 Void 1037

8.7.12 LAA 1037

8.7.12.1 FDD CA in licensed bands 1037

8.7.12.2 TDD CA in licensed bands 1039

8.7.12.3 TDD-FDD CA in licensed bands 1041

8.7.13 FDD DC (4 Rx) 1044

8.7.14 TDD DC (4 Rx) 1045

8.7.15 TDD FDD DC (4 Rx) 1047

8.7.16 FDD (1024QAM and up to 4Rx supported) 1049

8.7.17 TDD (1024QAM and up to 4 Rx supported) 1052

8.7.18 TDD FDD CA (1024QAM and up to 4 Rx supported) 1054

8.7.19 TDD (8 Rx) 1056

8.8 Demodulation of EPDCCH 1058

8.8.1 Distributed Transmission 1058

8.8.1.1 FDD 1058

8.8.1.1.1 Void 1059

8.8.1.2 TDD 1059

8.8.1.2.1 Void 1060

8.8.2 Localized Transmission with TM9 1060

8.8.2.1 FDD 1060

8.8.2.1.1 Void 1061

8.8.2.1.2 Void 1062

8.8.2.2 TDD 1062

8.8.2.2.1 Void 1063

8.8.2.2.2 Void 1063

8.8.3 Localized transmission with TM10 Type B quasi co-location type 1063

8.8.3.1 FDD 1063

8.8.3.2 TDD 1066

8.8.4 Enhanced Downlink Control Channel Performance Requirements Type A - Localized Transmission with CRS Interference Model 1069

8.8.4.1 FDD 1069

8.8.4.2 TDD 1070

8.8.5 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM9 Interference Model 1072

8.8.5.1 TDD 1072

8.8.6 Enhanced Downlink Control Channel Performance Requirements Type A - Distributed Transmission with TM3 Interference Model 1073

8.8.6.1 FDD 1073

8.9 Demodulation (single receiver antenna) 1074

8.9.1 PDSCH 1074

8.9.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1074

8.9.1.1.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1074

8.9.1.1.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1075

8.9.1.1.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1077

8.9.1.2 TDD (Fixed Reference Channel) 1080

8.9.1.2.1 Transmit diversity performance (Cell-Specific Reference Symbols) 1080

8.9.1.2.2 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1081

8.9.1.2.3 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1084

8.9.2 PHICH 1086

8.9.2.1 FDD and half-duplex FDD 1086

8.9.2.1.1 Transmit diversity performance 1086

8.9.2.2 TDD 1086

8.9.2.2.1 Transmit diversity performance 1086

8.9.3 PBCH 1087

8.9.3.1 FDD and half-duplex FDD 1087

8.9.3.1.1 Transmit diversity performance 1087

8.9.3.2 TDD 1087

8.9.3.2.1 Transmit diversity performance 1087

8.9.4 PDCCH/PCFICH 1087

8.9.4.1 FDD and half-duplex FDD 1087

8.9.4.1.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1087

8.9.4.1.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1088

8.9.4.2 TDD 1089

8.9.4.2.1 Enhanced Downlink Control Channel Performance Requirement Type A - 2 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1089

8.9.4.2.2 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1090

8.10 Demodulation (4 receiver antenna ports) 1091

8.10.1 PDSCH 1091

8.10.1.1 FDD (Fixed Reference Channel) 1091

8.10.1.1.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1092

8.10.1.1.1A Transmit diversity performance wit Enhanced Performance Requirement Type A - 2 Tx Antenna Ports with TM3 interference model 1093

8.10.1.1.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1094

8.10.1.1.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1094

8.10.1.1.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Port (Cell-Specific Reference Symbols) 1095

8.10.1.1.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1096

8.10.1.1.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1097

8.10.1.1.5A Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1100

8.10.1.1.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1101

8.10.1.1.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1102

8.10.1.1.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1104

8.10.1.1.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1105

8.10.1.1.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1106

8.10.1.1.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1106

8.10.1.1.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas (Cell-Specific Reference Symbols) 1107

8.10.1.1.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1107

8.10.1.1.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1109

8.10.1.1.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1110

8.10.1.1.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1111

8.10.1.1.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1112

8.10.1.1.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1113

8.10.1.1.14 HST-SFN performance 1117

8.10.1.2 TDD (Fixed Reference Channel) 1117

8.10.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1118

8.10.1.2.1A Transmit diversity performance with Enhanced Performance Requirement Type A – 2 Tx Antenna Ports with TM3 interference model 1119

8.10.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1120

8.10.1.2.3 Closed-loop spatial multiplexing Enhanced Performance Requirements Type A - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1120

8.10.1.2.4 Closed-loop spatial multiplexing performance, Dual-Layer Spatial Multiplexing 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1121

8.10.1.2.4A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing with 2Tx Antenna Ports 1122

8.10.1.2.5 Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1123

8.10.1.2.5A Single-layer Spatial Multiplexing (with multiple CSI-RS configurations) 1126

8.10.1.2.5B Single-layer Spatial Multiplexing (With Enhanced DMRS table configured) 1127

8.10.1.2.6 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1128

8.10.1.2.6A Enhanced Performance Requirement Type C - Dual-Layer Spatial Multiplexing 1130

8.10.1.2.6B Dual-Layer Spatial Multiplexing with altCQI-Table-1024QAM configured (User-Specific Reference Symbols) 1131

8.10.1.2.7 Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1132

8.10.1.2.7A Enhanced Performance Requirement Type C - Open-loop spatial multiplexing, 3 Layer Multiplexing with 4 Tx Antenna Ports (Cell-Specific Reference Symbols) 1132

8.10.1.2.8 Closed-loop spatial multiplexing performance, 4 Layers spatial multiplexing 4 Tx antennas 1133

8.10.1.2.9 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1134

8.10.1.2.9A Enhanced Performance Requirement Type C - 4 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1135

8.10.1.2.10 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 2 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1136

8.10.1.2.11 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing 4 Tx Antenna Port with CRS assistance information (Cell-Specific Reference Symbols) 1138

8.10.1.2.12 Closed loop spatial multiplexing performance - Single-Layer Spatial Multiplexing with CRS assistance information (User-Specific Reference Symbols) 1139

8.10.1.2.13 Performance requirements for DCI format 2D and non Quasi Co-located Antenna Ports 1140

8.10.1.2.14 HST-SFN performance 1144

8.10.2 PDCCH/PCFICH 1145

8.10.2.1 FDD 1145

8.10.2.1.1 Single-antenna port performance 1145

8.10.2.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1145

8.10.2.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1145

8.10.2.1.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1146

8.10.2.2 TDD 1147

8.10.2.2.1 Single-antenna port performance 1147

8.10.2.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1148

8.10.2.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1148

8.10.2.2.4 Enhanced Downlink Control Channel Performance Requirement Type A - 4 Tx Antenna Port with Non-Colliding CRS Dominant Interferer 1148

8.10.3 PHICH 1149

8.10.3.1 FDD 1149

8.10.3.1.1 Single Tx Antenna Port performance 1150

8.10.3.1.2 Transmit diversity performance with 2 Tx Antenna Ports 1150

8.10.3.1.3 Transmit diversity performance with 4 Tx Antenna Ports 1150

8.10.3.2 TDD 1151

8.10.3.2.1 Single Tx Antenna Port performance 1151

8.10.3.2.2 Transmit diversity performance with 2 Tx Antenna Ports 1152

8.10.3.2.3 Transmit diversity performance with 4 Tx Antenna Ports 1152

8.10.4 ePDCCH 1152

8.10.4.1 Distributed Transmission with 4Rx 1152

8.10.4.1.1 FDD 1152

8.10.4.1.2 TDD 1153

8.10.4.2 Localized Transmission with TM9 and 4Rx 1154

8.10.4.2.1 FDD 1154

8.10.4.2.2 TDD 1155

8.11 Demodulation (UE supporting coverage enhancement) 1156

8.11.1 PDSCH 1157

8.11.1.1 FDD and half-duplex FDD (Fixed Reference Channel) 1157

8.11.1.1.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1157

8.11.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1161

8.11.1.1.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1163

8.11.1.2 TDD (Fixed Reference Channel) 1169

8.11.1.2.1 Closed-loop spatial multiplexing performance (Cell-Specific Reference Symbols) 1169

8.11.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Symbols) 1174

8.11.1.2.3 Transmit diversity performance (Cell-Specific Reference Symbols) 1176

8.11.2 MPDCCH 1180

8.11.2.1 FDD and half-duplex FDD 1181

8.11.2.1.1 CE Mode A 1182

8.11.2.1.2 CE Mode B 1183

8.11.2.1.3 CE Mode A with TM9 interference model 1183

8.11.2.1.4 CE Mode A with CRS interference model 1185

8.11.2.1.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1186

8.11.2.2.5 CE Mode A and CE Mode B when CRS-ChEstMPDCCH-Config is configured 1187

8.11.2.2 TDD 1189

8.11.2.2.1 CE Mode A 1190

8.11.2.2.2 CE Mode B 1191

8.11.2.2.3 CE Mode A with TM9 interference model 1191

8.11.2.2.4 CE Mode A with CRS interference model 1192

8.11.3 PBCH 1193

8.11.3.1 FDD and half-duplex FDD 1194

8.11.3.1.1 Transmit diversity performance 1194

8.11.3.2 TDD 1195

8.11.3.2.1 Transmit diversity performance 1195

8.12 Demodulation of Narrowband IoT 1195

8.12.1 NPDSCH 1195

8.12.1.1.1 Minimum Requirements for In-band 1196

8.12.1.1.2 Minimum Requirements for Standalone/Guard-band 1197

8.12.1.1.3 Minimum Requirements for Standalone for UE Category NB2 1198

8.12.1.1.4 Minimum Requirements for Standalone for UE with multiple TBs interleaved transmission 1199

8.12.1.1.5 Minimum Requirements for Standalone for UE with 16-QAM 1199

8.12.1.2 TDD 1201

8.12.1.2.1 Minimum Requirements for In-band 1201

8.12.1.2.2 Minimum Requirements for Standalone/Guard-band 1202

8.12.1.2.3 Minimum Requirements for Standalone for UE Category NB2 1203

8.12.1.2.4 Minimum Requirements for Standalone for UE with 16-QAM 1203

8.12.2 NPDCCH 1204

8.12.2.1 Half-duplex FDD 1204

8.12.2.1.1 Single-antenna performance 1205

8.12.2.1.2 Transmit diversity performance 1206

8.12.2.2 TDD 1206

8.12.2.2.1 Single-antenna performance 1208

8.12.2.2.2 Transmit diversity performance 1208

8.12.3 Demodulation of NPBCH 1208

8.12.3.1 HD-FDD 1209

8.12.3.1.1 Single-antenna port performance with single NPBCH TTI 1209

8.12.3.1.2 Transmit diversity performance 1209

8.12.3.2 TDD 1209

8.12.3.2.1 Single-antenna port performance with single NPBCH TTI 1210

8.12.3.2.2 Transmit diversity performance 1210

8.13 Demodulation of PDSCH CA and DC(4 receiver antenna ports) 1210

8.13.1 FDD (CA and DC) 1210

8.13.1.1 Closed-loop spatial multiplexing performance 1210

8.13.1.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1210

8.13.1.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1214

8.13.1.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1216

8.13.1.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1218

8.13.1.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1219

8.13.1.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1219

8.13.1.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1222

8.13.1.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) 1222

8.13.1.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1224

8.13.1.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1224

8.13.2 TDD (CA and DC) 1227

8.13.2.1 Closed-loop spatial multiplexing performance 1228

8.13.2.1.1 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port 1228

8.13.2.1.2 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port for dual connectivity 1230

8.13.2.1.3 Minimum Requirement Multi-Layer Spatial Multiplexing 4 Tx Antenna Port with 256QAM 1231

8.13.2.1.4 Minimum Requirement Four-Layer Spatial Multiplexing 4 Tx Antenna Port 1232

8.13.2.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1234

8.13.2.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port 1234

8.13.2.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1238

8.13.2.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) 1238

8.13.3 TDD-FDD (CA and DC) 1240

8.13.3.1 Closed-loop spatial multiplexing performance 4Tx Antenna Port 1240

8.13.3.1.1 Minimum Requirement for FDD PCell 1240

8.13.3.1.2 Minimum Requirement for TDD PCell 1244

8.13.3.2 Dual-Layer Spatial Multiplexing (User-Specific Reference Symbols) 1248

8.13.3.2.1 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for FDD PCell 1248

8.13.3.2.2 Minimum Requirement Dual-Layer Spatial Multiplexing 2 Tx Antenna Port for TDD PCell 1251

8.13.3.3 Enhanced Performance Requirements Type A Closed-loop spatial multiplexing 1254

8.13.3.3.1 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for FDD PCell 1254

8.13.3.3.2 Minimum Requirement Single-Layer Spatial Multiplexing 2 Tx Antenna Port with TM4 interference model (Cell-Specific Reference Symbols) for TDD PCell 1256

8.13.3.4 Enhanced Performance Requirement Type A - Single-layer Spatial Multiplexing (User-Specific Reference Symbols) 1258

8.13.3.4.1 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for FDD PCell 1258

8.13.3.4.2 Minimum Requirement Enhanced Performance Requirement Type A – Single-layer Spatial Multiplexing with TM9 interference model (User-Specific Reference Symbols) for TDD PCell 1261

8.13.3.5 Closed-loop spatial multiplexing performance 4Tx Antenna Port for DC 1264

8.13.3.5.1 Minimum Requirement for FDD PCell 1264

8.13.3.5.2 Minimum Requirement for TDD PCell 1266

8.13.3.6 Closed-loop spatial multiplexing performance 4Tx Antenna Port with 256QAM 1268

8.13.3.6.1 Minimum Requirement for FDD PCell 1268

8.13.3.6.2 Minimum Requirement for TDD PCell 1270

8.13.3.7 Closed-loop spatial multiplexing performance 4Tx Antenna Port with Four layers 1271

8.13.3.7.1 Minimum Requirement for FDD PCell 1271

8.13.3.7.2 Minimum Requirement for TDD PCell 1273

8.14 Demodulation (UE supporting Short TTI) 1275

8.14.1 Slot-PDSCH and Subslot-PDSCH 1275

8.14.1.1 FDD (Fixed Reference Channel) 1275

8.14.1.1.1 Open-loop spatial multiplexing performance 1275

8.14.1.1.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1276

8.14.1.2 TDD (Fixed Reference Channel) 1278

8.14.1.2.1 Open-loop spatial multiplexing performance 1278

8.14.1.2.2 Closed-loop spatial multiplexing performance (User-Specific Reference Signals) 1279

8.14.2 SPDCCH 1280

8.14.2.1 FDD 1280

8.14.2.1.1 Mimimum requirement 1281

8.14.2.2 TDD 1281

8.14.2.2.1 Mimimum requirement 1282

8.15 Demodulation (8 receiver antenna ports) 1283

8.15.1 PDSCH 1283

8.15.1.1 Void 1283

8.15.1.2 TDD (Fixed Reference Channel) 1283

8.15.1.2.1 Transmit diversity performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1283

8.15.1.2.2 Open-loop spatial multiplexing performance with 2Tx Antenna Ports (Cell-Specific Reference Symbols) 1284

8.15.1.2.3 8 Layer Spatial Multiplexing (User-Specific Reference Symbols) 1284

8.15.2 CA 1286

8.15.2.1 Void 1286

8.15.2.2 TDD 1286

8.15.2.2.1 Eight Layer Spatial Multiplexing (User-Specific Reference Symbols) 1286

9 Reporting of Channel State Information 1288

9.1 General 1288

9.1.1 Applicability of requirements 1288

9.1.1.1 Applicability of requirements for different channel bandwidths 1288

9.1.1.2 Applicability and test rules for different CA configurations and bandwidth combination sets 1288

9.1.1.2A Applicability and test rules for different TDD-FDD CA configurations and bandwidth combination sets 1289

9.1.1.3 Test coverage for different number of componenet carriers 1290

9.1.1.4 Applicability of performance requirements for 4Rx capable UEs 1290

9.1.1.4.1 Applicability rule and antenna connection for single carrier tests with 2Rx 1290

9.1.1.4.2 Applicability rule and antenna connection for CA tests with 2Rx 1292

9.1.1.4.3 Applicability rule and antenna connection for single carrier tests with 4Rx 1293

9.1.1.5 Applicability of requirements for UEs supporting coverage enhancement 1293

9.2 CQI reporting definition under AWGN conditions 1293

9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbols) 1293

9.2.1.1 FDD 1293

9.2.1.2 TDD 1294

9.2.1.3 FDD (CSI measurements in case two CSI subframe sets are configured) 1295

9.2.1.4 TDD (CSI measurements in case two CSI subframe sets are configured) 1298

9.2.1.5 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1301

9.2.1.6 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1304

9.2.1.7 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1307

9.2.1.8 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1308

9.2.1.9 FDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1308

9.2.1.10 TDD (Modulation and TBS index Table 3 and 4-bit CQI Table 4 are used) 1309

9.2.2 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1310

9.2.2.1 FDD 1310

9.2.2.2 TDD 1311

9.2.3 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1312

9.2.3.1 FDD 1312

9.2.3.1A FDD (With *channelMeasRestriction* configured) 1313

9.2.3.2 TDD 1314

9.2.3.2A TDD (With *channelMeasRestriction* configured) 1315

9.2.4 Minimum requirement PUCCH 1-1 (With Single CSI Process) 1316

9.2.4.1 FDD 1317

9.2.4.1A FDD (With *interferenceMeasRestriction* configured) 1319

9.2.4.2 TDD 1322

9.2.4.2A TDD (With *interferenceMeasRestriction* configured) 1325

9.2.5 Minimum requirement PUCCH 1-1 (when *csi-SubframeSet –r12* and *EIMTA-MainConfigServCell-r12* are configured) 1328

9.2.6 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1331

9.2.6.1 Frame structure type 3 with FDD Pcell 1331

9.2.6.2 Frame structure type 3 with TDD Pcell 1333

9.2.7 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1335

9.2.7.1 Frame structure type 3 wth FDD Pcell 1335

9.2.7.2 Frame structure type 3 wth TDD Pcell 1337

9.3 CQI reporting under fading conditions 1341

9.3.1 Frequency-selective scheduling mode 1341

9.3.1.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbols) 1341

9.3.1.1.1 FDD 1341

9.3.1.1.2 TDD 1342

9.3.1.1.3 FDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1343

9.3.1.1.4 TDD (CSI measurements in case two CSI subframe sets are configured and with CRS assistance information) 1347

9.3.1.1.5 TDD (when *csi-SubframeSet –r12* is configured) 1350

9.3.1.2 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1352

9.3.1.2.1 FDD 1352

9.3.1.2.2 TDD 1353

9.3.1.2.3 FDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1355

9.3.1.2.4 TDD (Modulation and TBS index Table 2 and 4-bit CQI Table 2 are used) 1356

9.3.1.2.5 Void 1357

9.3.1.2.6 TDD (when *csi-SubframeSet –r12* is configured with one CSI process) 1357

9.3.2 Frequency non-selective scheduling mode 1361

9.3.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1361

9.3.2.1.1 FDD 1361

9.3.2.1.2 TDD 1363

9.3.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1365

9.3.2.2.1 FDD 1365

9.3.2.2.2 TDD 1366

9.3.3 Frequency-selective interference 1368

9.3.3.1 Minimum requirement PUSCH 3-0 (Cell-Specific Reference Symbol) 1368

9.3.3.1.1 FDD 1368

9.3.3.1.2 TDD 1369

9.3.3.2 Void 1370

9.3.3.2.1 Void 1370

9.3.3.2.2 Void 1370

9.3.4 UE-selected subband CQI 1370

9.3.4.1 Minimum requirement PUSCH 2-0 (Cell-Specific Reference Symbols) 1370

9.3.4.1.1 FDD 1370

9.3.4.1.2 TDD 1371

9.3.4.2 Minimum requirement PUCCH 2-0 (Cell-Specific Reference Symbols) 1372

9.3.4.2.1 FDD 1372

9.3.4.2.2 TDD 1374

9.3.5 Additional requirements for enhanced receiver Type A 1376

9.3.5.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) 1376

9.3.5.1.1 FDD 1376

9.3.5.1.2 TDD 1377

9.3.5.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1380

9.3.5.2.1 FDD 1380

9.3.5.2.2 TDD 1383

9.3.6 Minimum requirement (With multiple CSI processes) 1386

9.3.6.1 FDD 1387

9.3.6.2 TDD 1391

9.3.7 Minimum requirement PUSCH 3-2 1395

9.3.7.1 FDD 1395

9.3.7.2 TDD 1396

9.3.8 Additional requirements for enhanced receiver Type B 1398

9.3.8.1 Minimum requirement PUCCH 1-1 (Cell-Specific Reference Symbols) 1398

9.3.8.1.1 FDD 1398

9.3.8.1.2 TDD 1399

9.3.8.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbols) 1401

9.3.8.2.1 FDD 1401

9.3.8.2.2 TDD 1403

9.3.8.3 Minimum requirement with CSI process 1406

9.3.8.3.1 FDD 1406

9.3.8.3.2 TDD 1409

9.4 Reporting of Precoding Matrix Indicator (PMI) 1412

9.4.1 Single PMI 1413

9.4.1.1 Minimum requirement PUSCH 3-1 (Cell-Specific Reference Symbols) 1413

9.4.1.1.1 FDD 1413

9.4.1.1.2 TDD 1414

9.4.1.2 Minimum requirement PUCCH 2-1 (Cell-Specific Reference Symbols) 1415

9.4.1.2.1 FDD 1415

9.4.1.2.2 TDD 1417

9.4.1.3 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1418

9.4.1.3.1 FDD 1418

9.4.1.3.2 TDD 1421

9.4.1.3.3 FDD (with Class A 12Tx codebook) 1424

9.4.1.3.4 TDD (with Class A 12Tx codebook) 1426

9.4.1.3.5 FDD (with Class A 24Tx codebook) 1429

9.4.1.3.6 TDD (with Class A 24Tx codebook) 1431

9.4.1.4 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) 1434

9.4.1.4.1 FDD (with 4Tx enhanced codebook) 1434

9.4.1.4.2 TDD (with 4Tx enhanced codebook) 1436

9.4.1.4.3 FDD (with Class B alternative codebook for one CSI-RS resource configured) 1439

9.4.1.4.4 TDD (with Class B alternative codebook for one CSI-RS resource configured) 1441

9.4.1a Void 1444

9.4.1a.1 Void 1444

9.4.1a.1.1 Void 1444

9.4.1a.1.2 Void 1444

9.4.2 Multiple PMI 1444

9.4.2.1 Minimum requirement PUSCH 1-2 (Cell-Specific Reference Symbols) 1444

9.4.2.1.1 FDD 1444

9.4.2.1.2 TDD 1445

9.4.2.2 Minimum requirement PUSCH 2-2 (Cell-Specific Reference Symbols) 1446

9.4.2.2.1 FDD 1446

9.4.2.2.2 TDD 1447

9.4.2.3 Minimum requirement PUSCH 1-2 (CSI Reference Symbol) 1448

9.4.2.3.1 FDD 1448

9.4.2.3.2 TDD 1450

9.4.2.3.3 FDD (with 4Tx enhanced codebook) 1453

9.4.2.3.4 TDD (with 4Tx enhanced codebook) 1455

9.4.2.3.5 FDD (with Class A 16Tx codebook) 1457

9.4.2.3.6 TDD (with Class A 16Tx codebook) 1460

9.4.2.3.7 FDD (with Class A 32Tx codebook) 1463

9.4.2.3.8 TDD (with Class A 32Tx codebook) 1466

9.4.2.3.9 FDD (with Class A 16Tx advanced codebook) 1469

9.4.2.3.10 TDD (with Class A 16Tx advanced codebook) 1472

9.4.3 Void 1475

9.5 Reporting of Rank Indicator (RI) 1475

9.5.1 Minimum requirement (Cell-Specific Reference Symbols) 1475

9.5.1.1 FDD 1475

9.5.1.2 TDD 1476

9.5.2 Minimum requirement (CSI Reference Symbols) 1477

9.5.2.1 FDD 1477

9.5.2.2 TDD 1479

9.5.3 Minimum requirement (CSI measurements in case two CSI subframe sets are configured) 1481

9.5.3.1 FDD 1481

9.5.3.2 TDD 1484

9.5.4 Minimum requirement (CSI measurements in case two CSI subframe sets are configured and CRS assistance information are configured) 1487

9.5.4.1 FDD 1487

9.5.4.2 TDD 1490

9.5.5 Minimum requirement (with CSI process) 1493

9.5.5.1 FDD 1494

9.5.5.2 TDD 1497

9.6 Additional requirements for carrier aggregation 1500

9.6.1 Periodic reporting on multiple cells (Cell-Specific Reference Symbols) 1500

9.6.1.1 FDD 1500

9.6.1.2 TDD 1506

9.6.1.3 TDD-FDD CA with FDD PCell 1512

9.6.1.4 TDD-FDD CA with TDD PCell 1517

9.7 CSI reporting (Single receiver antenna) 1523

9.7.1 CQI reporting definition under AWGN conditions 1524

9.7.1.1 FDD and half-duplex FDD 1524

9.7.1.2 TDD 1524

9.7.1.3 FDD (Category 1bis UE) 1525

9.7.1.4 TDD (Category 1bis UE) 1526

9.7.2 CQI reporting under fading conditions 1527

9.7.2.1 FDD and half-duplex FDD 1527

9.7.2.2 TDD 1528

9.7.2.3 FDD (Category 1bis UE) 1529

9.7.2.4 TDD (Category 1bis UE) 1530

9.8 CSI reporting (UE supporting coverage enhancement) 1531

9.8.1 CQI reporting definition under AWGN conditions 1531

9.8.1.1 FDD and half-duplex FDD 1531

9.8.1.2 TDD 1532

9.8.2 UE-selected subband CQI 1533

9.8.2.1 FDD and half-duplex FDD 1533

9.8.2.2 TDD 1537

9.8.3 CQI reporting definition for UE supporting 64QAM under AWGN 1540

9.8.3.1 FDD and half-duplex FDD 1540

9.8.3.2 TDD 1541

9.8.4 CQI reporting definition for UE supporting alternative table under AWGN 1542

9.8.4.1 FDD and half-duplex FDD 1542

9.8.4.2 TDD 1543

9.8.5 PMI reporting with PUCCH 1-1 (CSI Reference Symbol) 1544

9.8.5.1 FDD 1545

9.8.5.2 TDD 1546

9.9 CSI reporting for 4Rx UE 1547

9.9.1 CQI reporting definition under AWGN conditions 1547

9.9.1.1 Minimum requirement PUCCH 1-0 with Rank 1 (Cell-Specific Reference Symbols) 1548

9.9.1.1.1 FDD 1548

9.9.1.1.2 TDD 1548

9.9.1.2 Minimum requirement PUCCH 1-1 with Rank 2 (CSI Reference Symbols) 1549

9.9.1.2.1 FDD 1549

9.9.1.2.2 TDD 1550

9.9.1.3 Minimum requirement PUCCH 1-1 with Rank 4 (Cell-Specific Reference Symbols) 1551

9.9.1.3.1 FDD 1552

9.9.1.3.2 TDD 1552

9.9.1.4 Minimum requirement PUCCH 1-1 with Rank 3 (CSI Reference Symbols) 1553

9.9.1.4.1 FDD 1553

9.9.1.4.2 TDD 1554

9.9.2 CQI reporting definition under fading conditions 1555

9.9.2.1 Minimum requirement PUCCH 1-0 (Cell-Specific Reference Symbol) for enhanced receiver Type A 1555

9.9.2.1.1 FDD 1556

9.9.2.1.2 TDD 1557

9.9.2.2 Minimum requirement PUCCH 1-1 (CSI Reference Symbol) for enhanced receiver Type A 1560

9.9.2.2.1 FDD 1560

9.9.2.2.2 TDD 1563

9.9.3 Reporting of Precoding Matrix Indicator (PMI) for 4Rx UE 1566

9.9.3.1 Minimum requirement PUSCH 3-1 (CSI Reference Symbol) 1567

9.9.3.1.1 TDD 1567

9.9.4 Reporting of Rank Indicator (RI) 1569

9.9.4.1 Minimum requirement (Cell-Specific Reference Symbols) 1569

9.9.4.1.1 FDD 1569

9.9.4.1.2 TDD 1571

9.9.4.2 Minimum requirement (CSI Reference Symbols) 1572

9.9.4.2.1 FDD 1572

9.9.4.2.2 TDD 1574

9.10 Reporting of CSI-RS Resource Indicator (CRI) 1576

9.10.1 Minimum requirement (PUSCH 3-1) 1577

9.10.1.1 FDD 1577

9.10.1.2 TDD 1579

9.10.2 Minimum requirement (PUSCH 3-1, QCL Type C) 1581

9.10.2.1 FDD 1581

9.10.2.2 TDD 1584

9.11 Reporting of Hybrid Channel state information 1587

9.11.1 Minimum requirement (with eMIMO-Type configured as Class B with more than one CSI-RS resource configured and eMIMO-Type2 as Class B with one CSI-RS resource configured) 1587

9.11.1.1 FDD 1588

9.11.1.2 TDD 1590

9.12 CSI reporting (UE supporting Short TTI) 1592

9.12.1 CQI reporting under fading conditions (Cell-Specific Reference Symbol) 1592

9.12.1.1 FDD 1592

9.12.1.2 TDD 1595

9.12.2 CQI reporting under fading conditions (CSI Reference Symbol) 1596

9.12.2.1 FDD 1596

9.12.2.2 TDD 1599

9.13 CSI reporting for 8Rx UE 1601

9.13.1 CQI reporting definition under AWGN conditions 1601

9.13.1.1 Minimum requirement PUCCH 1-1 with Rank 4 (CSI Reference Symbols) 1601

9.13.1.2.1 Void 1601

9.13.1.2.2 TDD 1601

9.14 CSI reporting of Narrowband IoT 1602

9.14.1 CQI reporting definition under AWGN conditions 1602

9.14.1.1 Half-duplex FDD 1602

9.14.1.2 TDD 1603

10 Performance requirement (MBMS) 1604

10.1 FDD (Fixed Reference Channel) 1604

10.1.1 Minimum requirement 1605

10.2 TDD (Fixed Reference Channel) 1606

10.2.1 Minimum requirement 1606

10.3 FDD (Fixed Reference Channel) with FeMBMS 1607

10.3.1 Minimum requirement for FeMBMS Unicast-mixed Cell under CA 1607

10.3.1.1 Minimum requirement with 1.25kHz subcarrier spacing 1607

10.3.1.2 Minimum requirement with 7.5kHz subcarrier spacing 1608

10.3.2 Minimum requirement for FeMBMS Unicast-mixed Cell as Non-Serving Cell 1609

10.3.2.1 Minimum requirement with 1.25kHz subcarrier spacing 1609

10.3.2.2 Minimum requirement with 7.5kHz subcarrier spacing 1610

10.3.3 Minimum requirement for MBMS Dedicated cell 1611

10.3.3.1 Minimum requirement with 1.25kHz subcarrier spacing 1611

10.3.3.2 Minimum requirement with 7.5kHz subcarrier spacing 1612

10.3.3.3 Minimum requirement with 15kHz subcarrier spacing 1613

10.4 FDD with 5G terrestrial broadcast 1614

10.4.1 Minimum requirement for PMCH decoding 1614

10.4.1.1 Minimum requirement with 0.37kHz subcarrier spacing 1614

10.4.1.2 Minimum requirement with 2.5kHz subcarrier spacing 1616

10.4.2 Minimum requirement for CAS detection 1617

10.4.2.1 Minimum requirement for PBCH detection 1617

11 Performance requirement (ProSe Direct Discovery) 1618

11.1 General 1618

11.1.1 Applicability of requirements 1618

11.1.2 Reference DRX configuration 1619

11.2 Demodulation of PSDCH (single link performance) 1619

11.2.1 FDD (in-coverage) 1619

11.2.2 TDD (in-coverage) 1620

11.2.3 FDD (out-of-coverage) 1621

11.3 Power imbalance performance with two links 1621

11.3.1 FDD 1621

11.3.2 TDD 1622

11.4 Multiple timing reference test 1623

11.4.1 FDD 1624

11.5 Maximum Sidelink processes test 1625

11.5.1 FDD 1625

11.5.2 TDD 1626

12 Performance requirement (ProSe Direct Communication) 1628

12.1 General 1628

12.1.1 Applicability of requirements 1628

12.1.1.1 Applicability of requirements for different channel bandwidths 1628

12.1.1.2 Test coverage for different number of component carriers 1628

12.1.1.3 Applicability and test rules for different CA configurations and bandwidth combination sets 1628

12.1.2 Reference DRX configuration 1629

12.2 Demodulation of PSSCH 1629

12.2.1 FDD 1629

12.3 Demodulation of PSCCH 1630

12.3.1 FDD 1631

12.4 Demodulation of PSBCH 1632

12.4.1 FDD 1632

12.5 Power imbalance performance with two links 1632

12.5.1 FDD 1632

12.6 Multiple timing reference test 1634

12.6.1 FDD 1634

12.7 Maximum Sidelink processes test 1637

12.7.1 FDD 1637

12.8 Sustained downlink data rate with active Sidelink 1638

13 Void 1640

14 Performance requirement (V2X Sidelink Communication) 1640

14.1 General 1640

14.1.1 Applicability of requirements 1640

14.2 Demodulation of PSSCH 1641

14.3 Demodulation of PSCCH 1642

14.4 Power imbalance performance with two links 1642

14.5 Demodulation of PSBCH 1643

14.6 Demodulation of PSSCH with eNB based synchronization 1644

14.7 Soft buffer test 1644

14.8 PSCCH/PSSCH decoding capability test 1645

14.9 Sustained downlink data rate with active sidelink 1646

14.10 Soft buffer test (CA) 1647

14.11 PSCCH/PSSCH decoding capability test (CA) 1648

Annex A (normative): Measurement channels 1646

A.1 General 1646

A.2 UL reference measurement channels 1646

A.2.1 General 1646

A.2.1.1 Applicability and common parameters 1646

A.2.1.2 Determination of payload size 1646

A.2.1.3 Overview of UL reference measurement channels 1647

A.2.2 Reference measurement channels for FDD 1670

A.2.2.1 Full RB allocation 1670

A.2.2.1.1 QPSK 1670

A.2.2.1.2 16-QAM 1672

A.2.2.1.3 64-QAM 1674

A.2.2.1.4 256 QAM 1675

A.2.2.2 Partial RB allocation 1675

A.2.2.2.1 QPSK 1676

A.2.2.2.2 16-QAM 1679

A.2.2.2.3 64-QAM 1681

A.2.2.2.4 256 QAM 1683

A.2.2.3 Void 1683

A.2.2.4 subPRB allocation 1684

A.2.3 Reference measurement channels for TDD 1684

A.2.3.1 Full RB allocation 1684

A.2.3.1.1 QPSK 1684

A.2.3.1.2 16-QAM 1687

A.2.3.1.3 64-QAM 1689

A.2.3.1.4 256 QAM 1690

A.2.3.2 Partial RB allocation 1690

A.2.3.2.1 QPSK 1691

A.2.3.2.2 16-QAM 1695

A.2.3.2.3 64-QAM 1700

A.2.3.2.4 256 QAM 1702

A.2.3.3 Void 1702

A.2.3.4 subPRB allocation 1703

A.2.4 Reference measurement channels for UE category NB1 1703

A.2.5 Reference measurement channels for LAA 1704

A.2.5.1 Full RB allocation 1704

A.2.5.1.1 QPSK 1704

A.2.5.1.2 16QAM 1705

A.2.5.1.3 64QAM 1705

A.2.5.2 Partial RB allocation 1705

A.2.5.2.1 QPSK 1706

A.2.5.2.2 16QAM 1706

A.2.5.2.3 64QAM 1707

A.3 DL reference measurement channels 1707

A.3.1 General 1707

A.3.1.1 Overview of DL reference measurement channels 1708

A.3.2 Reference measurement channel for receiver characteristics 1733

A.3.3 Reference measurement channels for PDSCH performance requirements (FDD) 1763

A.3.3.1 Single-antenna transmission (Common Reference Symbols) 1763

A.3.3.2 Multi-antenna transmission (Common Reference Symbols) 1768

A.3.3.2.1 Two antenna ports 1768

A.3.3.2.2 Four antenna ports 1777

A.3.3.3 Reference Measurement Channel for UE-Specific Reference Symbols 1782

A.3.3.3.0 Two antenna ports (no CSI-RS) 1782

A.3.3.3.1 Two antenna port (CSI-RS) 1783

A.3.3.3.2 Four antenna ports (CSI-RS) 1786

A.3.3.3.2A Eight antenna ports (CSI-RS) 1793

A.3.3.3.3 Twelve antenna port (CSI-RS) 1795

A.3.3.3.4 Sixteen antenna port (CSI-RS) 1796

A.3.3.3.5 Twenty-four antenna port (CSI-RS) 1797

A.3.3.3.6 Thirty-two antenna port (CSI-RS) 1798

A.3.4 Reference measurement channels for PDSCH performance requirements (TDD) 1800

A.3.4.1 Single-antenna transmission (Common Reference Symbols) 1800

A.3.4.2 Multi-antenna transmission (Common Reference Signals) 1808

A.3.4.2.1 Two antenna ports 1808

A.3.4.2.2 Four antenna ports 1821

A.3.4.3 Reference Measurement Channels for UE-Specific Reference Symbols 1828

A.3.4.3.1 Single antenna port (Cell Specific) 1828

A.3.4.3.2 Two antenna ports (Cell Specific) 1829

A.3.4.3.3 Two antenna ports (CSI-RS) 1831

A.3.4.3.4 Four antenna ports (CSI-RS) 1839

A.3.4.3.5 Eight antenna ports (CSI-RS) 1846

A.3.4.3.6 Twelve antenna ports (CSI-RS) 1852

A.3.4.3.7 Sixteen antenna ports (CSI-RS) 1853

A.3.4.3.8 Twenty-four antenna ports (CSI-RS) 1854

A.3.4.3.9 Thirty-two antenna ports (CSI-RS) 1855

A.3.5 Reference measurement channels for PDCCH/PCFICH performance requirements 1857

A.3.5.1 FDD 1857

A.3.5.2 TDD 1857

A.3.5.3 LAA 1858

A.3.6 Reference measurement channels for PHICH performance requirements 1858

A.3.7 Reference measurement channels for PBCH performance requirements 1858

A.3.8 Reference measurement channels for MBMS performance requirements 1859

A.3.8.1 FDD 1859

A.3.8.2 TDD 1864

A.3.9 Reference measurement channels for sustained downlink data rate provided by lower layers 1866

A.3.9.1 FDD 1866

A.3.9.2 TDD 1870

A.3.9.3 FDD (EPDCCH scheduling) 1884

A.3.9.4 TDD (EPDCCH scheduling) 1885

A.3.9.5 LAA 1887

A.3.10 Reference Measurement Channels for EPDCCH performance requirements 1889

A.3.10.1 FDD 1889

A.3.10.2 TDD 1889

A.3.11 Reference Measurement Channels for MPDCCH performance requirements 1889

A.3.11.1 FDD and half-duplex FDD 1889

A.3.11.2 TDD 1890

A.3.12 Reference measurement channels for NPDSCH performance requirements 1891

A.3.12.1 In-band 1891

A.3.12.1.2 Two-antenna transmission 1891

A.3.12.2 Standalone/Guard-band 1893

A.3.12.2.1 Single-antenna transmission 1893

A.3.13 Reference measurement channels for NPDCCH performance requirements 1896

A.3.13.1 Half-duplex FDD 1896

A.3.13.2 TDD 1897

A.3.14 Reference measurement channels for NPBCH performance requirements for Cat NB1 UEs 1897

A.3.15 Reference Measurement Channels for LAA SCell with frame structure Type-3 1898

A.3.15.1 Multi-antenna transmission (Common Reference Symbols) 1898

A.3.15.1.1 Four antenna ports 1898

A.3.15.2 Reference Measurement Channel for UE-Specific Reference Symbols 1898

A.3.15.2.1 Two antenna ports (CSI-RS) 1898

A.3.16 Reference measurement channels for Slot-PDSCH and Subslot-PDSCH performance requirements 1900

A.3.16.1 FDD 1900

A.3.16.2 TDD 1904

A.3.17 Reference measurement channels for SPDCCH performance requirements 1905

A.3.17.1 FDD 1905

A.3.17.2 TDD 1906

A.3.18 Reference Measurement Channels for LTE based 5G broadcast PMCH receiver requirements 1906

A.3.18.1 SDO 1906

A.4 CSI reference measurement channels 1908

A.5 OFDMA Channel Noise Generator (OCNG) 1923

A.5.1 OCNG Patterns for FDD 1923

A.5.1.1 OCNG FDD pattern 1: One sided dynamic OCNG FDD pattern 1923

A.5.1.2 OCNG FDD pattern 2: Two sided dynamic OCNG FDD pattern 1924

A.5.1.3 OCNG FDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1924

A.5.1.3A OCNG FDD pattern 3A: 49 RB OCNG allocation with MBSFN enhancement in 10 MHz 1925

A.5.1.4 OCNG FDD pattern 4: One sided dynamic OCNG FDD pattern for MBMS transmission 1925

A.5.1.4A OCNG FDD pattern 4A: One sided dynamic OCNG FDD pattern for enhanced MBMS transmission 1926

A.5.1.5 OCNG FDD pattern 5: One sided dynamic 16QAM modulated OCNG FDD pattern 1927

A.5.1.6 OCNG FDD pattern 6: dynamic OCNG FDD pattern when user data is in 2 non-contiguous blocks 1928

A.5.1.8 OCNG FDD pattern 8: Dynamic OCNG FDD pattern for TM10 transmission 1929

A.5.2 OCNG Patterns for TDD 1930

A.5.2.1 OCNG TDD pattern 1: One sided dynamic OCNG TDD pattern 1930

A.5.2.2 OCNG TDD pattern 2: Two sided dynamic OCNG TDD pattern 1931

A.5.2.3 OCNG TDD pattern 3: 49 RB OCNG allocation with MBSFN in 10 MHz 1932

A.5.2.4 OCNG TDD pattern 4: One sided dynamic OCNG TDD pattern for MBMS transmission 1932

A.5.2.5 OCNG TDD pattern 5: One sided dynamic 16QAM modulated OCNG TDD pattern 1933

A.5.2.6 OCNG TDD pattern 6: dynamic OCNG TDD pattern when user data is in 2 non-contiguous blocks 1934

A.5.2.8 OCNG TDD pattern 8: Dynamic OCNG TDD pattern for TM10 transmission 1935

A.5.3 OCNG Patterns for Narrowband IoT 1936

A.5.3.1 Narrowband IoT OCNG pattern 1 1936

A.5.4 OCNG Patterns for frame structure type 3 1937

A.5.4.1 OCNG FS3 pattern 1: One sided dynamic OCNG frame structure type 3 pattern 1937

A.5.4.2 OCNG FS3 pattern 2: Two sided dynamic OCNG frame structure 3 pattern 1938

A.6 Sidelink reference measurement channels 1939

A.6.1 General 1939

A.6.1.1 Overview of ProSe reference measurement channels 1939

A.6.2 Reference measurement channel for receiver characteristics 1940

A.6.3 Reference measurement channels for PSDCH performance requirements 1942

A.6.4 Reference measurement channels for PSCCH performance requirements 1943

A.6.5 Reference measurement channels for PSSCH performance requirements 1943

A.6.6 Reference measurement channels for PSBCH performance requirements 1944

A.7 Sidelink reference resource pool configurations 1945

A.7.1 Reference resource pool configurations for ProSe Direct Discovery demodulation tests 1945

A.7.1.1 FDD 1945

A.7.1.2 TDD 1948

A.7.2 Reference resource pool configurations for ProSe Direct Communication demodulation tests 1950

A.7.2.1 FDD 1950

A.8 V2X reference measurement channels 1955

A.8.1 General 1955

A.8.1.1 Overview of V2X reference measurement channels 1956

A.8.2 Reference measurement channel for receiver characteristics 1956

A.8.3 Reference measurement channel for transmitter characteristics 1958

A.8.4 Reference measurement for PSCCH performance requirements 1961

A.8.5 Reference measurement for PSSCH performance requirements 1962

A.8.6 Reference measurement for PSBCH performance requirements 1962

A.9 V2X reference resource pool configurations 1963

Annex B (normative): Propagation conditions 1966

B.1 Static propagation condition 1966

B.1.1 UE Receiver with 2Rx 1966

B.1.2 UE Receiver with 4Rx 1966

B.1.3 UE Receiver with 8Rx 1967

B.2 Multi-path fading propagation conditions 1968

B.2.1 Delay profiles 1968

B.2.2 Combinations of channel model parameters 1969

B.2.3 MIMO Channel Correlation Matrices 1970

B.2.3.1 Definition of MIMO Correlation Matrices 1970

B.2.3.2 MIMO Correlation Matrices at High, Medium and Low Level 1976

B.2.3A MIMO Channel Correlation Matrices using cross polarized antennas 1979

B.2.3A.1 Definition of MIMO Correlation Matrices using cross polarized antennas 1980

B.2.3A.2 Spatial Correlation Matrices using cross polarized antennas at eNB and UE sides 1980

B.2.3A.2.1 Spatial Correlation Matrices at eNB side 1980

B.2.3A.2.2 Spatial Correlation Matrices at UE side 1981

B.2.3A.4 Beam steering approach 1984

B.2.3B MIMO Channel Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1984

B.2.3B.1 Definition of MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1985

B.2.3B.2 Spatial Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1986

B.2.3B.2.1 Spatial Correlation Matrices at eNB side 1986

B.2.3B.2.2 Spatial Correlation Matrices at UE side 1986

B.2.3B.3 MIMO Correlation Matrices using two-dimension cross polarized antennas at eNB and cross polarized antennas at UE 1986

B.2.3B.4 Beam steering approach 1989

B.2.3B.4A Beam steering approach with dual cluster beams 1990

B.2.4 Propagation conditions for CQI tests 1991

B.2.4.1 Propagation conditions for CQI tests with multiple CSI processes 1991

B.2.5 Void 1991

B.2.6 MBSFN Propagation Channel Profile 1991

B.2.6.1 Subcarrier spacing 15kHz or 7.5kHz 1991

B.2.6.2 Subcarrier spacing 1.25kHz 1992

B.2.6.3 Subcarrier spacing 0.37kHz 1993

B.2.6.4 Subcarrier spacing 2.5kHz 1993

B.3 High speed train scenario 1994

B.3A HST-SFN scenario 1995

B.3B HST-SFN scenario for 500 km/h speed 1999

B.3C HST scenario for 500 km/h speed 1999

B.4 Beamforming Model 1999

B.4.1 Single-layer random beamforming (Antenna port 5, 7, or 8) 1999

B.4.1A Single-layer random beamforming (Antenna port 7, 8, 11 or 13 with enhanced DMRS table configured) 2000

B.4.2 Dual-layer random beamforming (antenna ports 7 and 8) 2000

B.4.3 Generic beamforming model (antenna ports 7-14) 2001

B.4.4 Random beamforming for EPDCCH distributed transmission (Antenna port 107 and 109) 2002

B.4.5 Random beamforming for EPDCCH localized transmission (Antenna port 107, 108, 109 or 110) 2002

B.4.6 Beamforming model for CRI test 2002

B.5 Interference models for enhanced performance requirements Type-A 2004

B.5.1 Dominant interferer proportion 2004

B.5.2 Transmission mode 3 interference model 2004

B.5.3 Transmission mode 4 interference model 2004

B.5.4 Transmission mode 9 interference model 2005

B.6 Interference models for enhanced performance requirements Type-B 2005

B.6.1 Transmission mode 2 interference model 2005

B.6.2 Transmission mode 3 interference model 2006

B.6.3 Transmission mode 4 interference model 2006

B.6.4 Transmission mode 9 interference model 2006

B.6.5 CRS interference model 2007

B.6.6 Random interference model 2007

B.7 Interference models for enhanced downlink control channel performance requirements Type A and B 2008

B.7.1 PDCCH, PCFICH and PHICH interference model 2008

B.8 Burst transmission models for Frame structure type 3 2009

B.8.1 Burst transmission model for one LAA SCell 2009

B.8.2 Burst transmission model for multiple LAA SCell(s) 2009

Annex C (normative): Downlink Physical Channels 2011

C.1 General 2011

C.2 Set-up 2011

C.3 Connection 2011

C.3.1 Measurement of Receiver Characteristics 2011

C.3.2 Measurement of Performance requirements 2012

C.3.3 Aggressor cell power allocation for Measurement of Performance Requirements when ABS is Configured 2013

C.3.4 Power Allocation for Measurement of Performance Requirements when Quasi Co-location Type B: same Cell ID 2014

C.3.5 Simplified CA testing method 2014

C.3.6 Measurement of Receiver Characteristics for Narrowband IoT 2015

Annex D (normative): Characteristics of the interfering signal 2016

D.1 General 2016

D.2 Interference signals 2016

Annex E (normative): Environmental conditions 2017

E.1 General 2017

E.2 Environmental 2017

E.2.1 Temperature 2017

E.2.2 Voltage 2017

E.2.3 Vibration 2018

Annex F (normative): Transmit modulation 2019

F.1 Measurement Point 2019

F.2 Basic Error Vector Magnitude measurement 2019

F.3 Basic in-band emissions measurement 2020

F.4 Modified signal under test 2020

F.5 Window length 2022

F.5.1 Timing offset 2022

F.5.2 Window length 2022

F.5.3 Window length for normal CP 2022

F.5.4 Window length for Extended CP 2023

F.5.5 Window length for PRACH 2023

F.5.F Window length for category NB1 2024

F.6 Averaged EVM 2024

F.6.F Averaged EVM for category NB1 2025

F.7 Spectrum Flatness 2025

Annex G (informative): Reference sensitivity level in lower SNR 2026

G.1 General 2026

G.2 Typical receiver sensitivity performance (QPSK) 2026

G.3 Reference measurement channel for REFSENSE in lower SNR 2032

Annex H (normative): Modified MPR behavior 2035

H.1 Indication of modified MPR behavior 2035

Annex I (normative): Supported Post Antenna Gain 2036

I.1 Declared Supported Post Antenna Gain for UE 2036

Annex J (informative): Change history 2037